**SC-DP-II型提拉镀膜机**

名称：提拉镀膜机； 品牌：北京赛德凯斯；

厂家：北京赛德凯斯电子有限责任公司； 型号：SC-DP-II

公司网址：http://setcas.com/?page\_id=4772

|  |  |
| --- | --- |
| [/Users/hoyelam/Desktop/阿里巴巴國際站/阿里巴巴國際站所需資料/9.所有產品資料/5.提拉鍍膜機Dip Coater/2.SC-DP-II/1.SC-DP-II型提拉鍍膜機.jpeg1.SC-DP-II型提拉鍍膜機](http://setcas.com/wp-content/uploads/2020/12/%E7%AB%8B%E4%BD%93%E5%B0%8F.jpg) | [/Users/hoyelam/Desktop/阿里巴巴國際站/阿里巴巴國際站所需資料/9.所有產品資料/5.提拉鍍膜機Dip Coater/2.SC-DP-II/1.SC-DP-II型提拉鍍膜機.jpeg1.SC-DP-II型提拉鍍膜機](http://setcas.com/wp-content/uploads/2020/12/%E7%AB%8B%E4%BD%93%E5%B0%8F.jpg) |
| ****SC-DP-II型桌面型提拉镀膜机（加热）**** |
| **主要参数** | **指标** |
| 温度范围 | 室温-200℃ |
| 进样行程 | 300mm |
| 提拉速度范围 | 1um/s-20000um/s |
| 提拉分辨率 | 1um/s |
| 浸渍时间 | 0-9999S |
| 镀膜次数 | 1-9999次 |
| 每次镀膜间隔时间 | 0-9999S |
| 额定线性推力 | 20N |
| 控制精度 | ≤0.5% |

**SC-DP-II Table type of Dip Coater（heating）**

|  |  |
| --- | --- |
| [/Users/hoyelam/Desktop/阿里巴巴國際站/阿里巴巴國際站所需資料/9.所有產品資料/5.提拉鍍膜機Dip Coater/2.SC-DP-II/1.SC-DP-II型提拉鍍膜機.jpeg1.SC-DP-II型提拉鍍膜機](http://setcas.com/wp-content/uploads/2020/12/%E7%AB%8B%E4%BD%93%E5%B0%8F.jpg) | [/Users/hoyelam/Desktop/阿里巴巴國際站/阿里巴巴國際站所需資料/9.所有產品資料/5.提拉鍍膜機Dip Coater/2.SC-DP-II/1.SC-DP-II型提拉鍍膜機.jpeg1.SC-DP-II型提拉鍍膜機](http://setcas.com/wp-content/uploads/2020/12/%E7%AB%8B%E4%BD%93%E5%B0%8F.jpg) |
| ****SC-DP-II Table type of Dip Coater（heating）**** |
| **Main Parameter** | Index |
| Temperature range | Room temperature -200℃ |
| The operation process of lofting sample | 150mm |
| Speed range | 1um/s-20000um/s |
| Resolution | 1um/s |
| Immersion time | 0-9999S |
| Coating times | 1-9999 times |
| Time between each coating | 0-9999S |
| Rated linear thrust | 20N |
| Control precision | ≤0.5% |